**AFA Operations Specifications**

All pilots and instructors must adhere to the following conditions

\*Approval of exceptions must be made by Andrew Doremus\*

| AFA Wx  Specifications | Solo | Renter | Dual | Night |
| --- | --- | --- | --- | --- |
| Ceilings | Local – 5000’ ceiling  Anywhere Else – 3000’ ceiling | VFR Only | VFR Only | SCT @ ≥5000’  Moon ≥50% |
| Visibility | Local – 5SM  Anywhere else – 3SM | VFR Only | VFR Only | 5SM |
| Winds Aloft | Local – 12000’ @ 25kts  Anywhere else – 15000’ @ 40kts | 15000’ @ 40kts | 15000’ @ 50kts | Filed altitude not to exceed 25 kts |
| Max Wind | 10kts – includes instantaneous wind | 25kts – includes instantaneous wind | 30kts – includes instantaneous wind | 15kts – includes instantaneous wind |
| Direct X-Wind | 10kts – includes instantaneous wind | 20kts – includes instantaneous wind | 25kts – includes instantaneous wind | 10kts – includes instantaneous wind |
| Tailwind | 5kts – includes instantaneous wind | 10kts – includes instantaneous wind | 10kts – includes instantaneous wind | 5kts – includes instantaneous wind |

**1.** Night Solo Prohibited **6.** All Airmets must be verified before every flight

**2.** FICON (Field Condition) 4 or greater **7.** Minimum runway length 3000ft

**3.** Check out flight requires 1 hr. flight and 1 hr. ground & expires in 6 months **8.** Flight into snow or rain in an Airmet Zulu is prohibited

**4.** Must remain outside of Sigmets and Convective Sigmet borders **9.** Only paved runways

**5.** 15 Departures are prohibited **10.** Must land with 1 hr. of fuel remaining